Steel String guitar material list

* 1 - Indian rosewood back and sides 3A – I prefer dread size but OM size will work if making an OM [stewmac.sjv.io/5gvmbn](https://stewmac.sjv.io/5gvmbn)
* 1 - Sitka spruce top 3A – large enough for dread - [stewmac.sjv.io/0ZvXJ3](https://stewmac.sjv.io/0ZvXJ3)
* 1 - Ebony fretboard blank 1st grade approx. 2-3/8" x 20" x 15/64" - [stewmac.sjv.io/B033A9](https://stewmac.sjv.io/B033A9)
* 1 - Peghead veneer - one piece of ebony 3.5 inches X 7 inches approx. 3mm thick - [stewmac.sjv.io/xkKKX1](https://stewmac.sjv.io/xkKKX1%20%20)
* 1 - Peghead veneer maple veneer approx. .6mm thick of the same dimensions. ( you can find this at woodcraft, Rockler or other suppliers B&B Rarewoods is an excellent source for veneers - <https://www.dyed-veneer.com/>
* 1 - Mahogany neck blank 1st grade – approx. 7/8 inch - 1 inch X 3.25 inches X 35 inches [stewmac.sjv.io/zNoXNm](https://stewmac.sjv.io/zNoXNm)  **item 2593 or 2596**
* 1 - End block (Spanish cedar or mahogany) approx. 1 inch thick X 75mm to 80mm wide X 120mm tall. [stewmac.sjv.io/75vL53](https://stewmac.sjv.io/75vL53)
* 1 - Neck block mahogany approx. 32mm - 35mm thick X 75mm to 80 mm wide by 100 to 120mm tall [stewmac.sjv.io/75vL53](https://stewmac.sjv.io/75vL53)
* 4 - Flame maple bindings – ¼ inch tall X 2.25mm thick X 35 inches long (we can perhaps go with a different option here but clear with me first) [stewmac.sjv.io/q4akzO](https://stewmac.sjv.io/q4akzO)
* 1 End wedge blank that matches the binding material. I use flame maple when using flame maple bindings – approx. 2 inches wide X 6 inches long X 2.5mm to 3.5mm thick
* 3 B/W/B wood fiber laminate purfling .060 wide X .080 tall X 64 inches long [sjv.io/PyMYzq](https://stewmac.sjv.io/PyMYzq) **item 1765** You will need 4 of these if they are only 31.5 inches long. Some places have them in the 64 inch length.
* 1 Steel string herringbone rosette (Traditional Martin style) (other options can also work but clear with me first. A solid wood ring is also acceptable. [stewmac.sjv.io/QyMzK9](https://stewmac.sjv.io/QyMzK9)
* 4 Pieces of mahogany reversed kerfing. ( I prefer the reversed kerfing over the traditional) [stewmac.sjv.io/g1nnN5](https://stewmac.sjv.io/g1nnN5)  **item 4512** – (you will need 4 pieces)
* Fretwire for 20 frets 25.4mm scale length - [stewmac.sjv.io/WqeeJA](https://stewmac.sjv.io/WqeeJA) **item 0148** (you will need 3 pieces)
* 1 Ebony steel string bridge blank - 1st grade - [stewmac.sjv.io/xkgbZk](https://stewmac.sjv.io/xkgbZk) **item 0925**
* 1 - Back bracewood blank mahogany - [stewmac.sjv.io/xkgbZO](https://stewmac.sjv.io/xkgbZO) item 4658 WRC or item 4656 are okay if mahogany not available
* 2 - Top bracewood blank – Sitka spruce - [stewmac.sjv.io/xkgbZO](https://stewmac.sjv.io/xkgbZO) **item 4656** (spruce) you will need two pieces.
* 1 Steel string guitar bleached bone nut blank [stewmac.sjv.io/g1xNG0](https://stewmac.sjv.io/g1xNG0) **item 6020**
* 1 Steel string guitar bleached bone saddle blank [stewmac.sjv.io/anM6eQ](https://stewmac.sjv.io/anM6eQ) **item 6031**
* 6 Ebony slotted bridge pins - [stewmac.sjv.io/3evOZA](https://stewmac.sjv.io/3evOZA) I prefer **item 4975-S** but other options are available
* 1 - Cedar or spruce back reinforcement strip – approx 22 inches X ¾ inch wide X 3/32 thick – This can be made from the soundboard cutoff
* 1 set of Gotoh post tuners - gold or chrome with or without black knobs [stewmac.sjv.io/B0ve2B](https://stewmac.sjv.io/B0ve2B)
* 1 – Truss rod double action welded, 14 1/2" x 3/8" (overall length 15 1/2") [stewmac.sjv.io/xkgX2x](https://stewmac.sjv.io/xkgX2x) **item 2651**
* MOP Fret markers – ¼ diameter enough to do frets 3, 5, 7 , 9 12, 15, 17, 19 [stewmac.sjv.io/9g7xMY](https://stewmac.sjv.io/9g7xMY) **item 0011**
* white plastic side fret markers – [stewmac.sjv.io/ZQMJX01](https://stewmac.sjv.io/ZQMJX0) **item 0483**
* 1 - Roll binding tape - [stewmac.sjv.io/5gvLYD](https://stewmac.sjv.io/5gvLYD) **item 0584**
* 1 - Bottle of glue - [sjv.io/VmMVBJ](https://stewmac.sjv.io/VmMVBJ) **item 0622**
* 2 Furniture fasteners (2 barrel nuts and 2 bolts) Bolt ¼-20 X 30mm (1 3/16) - Barrel nut ¼-20 X 16mm (5/8) These are available at Lowes and Home Depot.